Defines | Functions | Variables

# UartDisplay.c File Reference

UartDisplay Main File. More...

`#include <avr/io.h>`
`#include <avr/interrupt.h>`
`#include <avr/pgmspace.h>`
`#include <util/delay.h>`
`#include <stdlib.h>`
`#include "lcd.h"`
`#include "uart.h"`
`#include "button.h"`
`#include "buzzer.h"`
Include dependency graph for UartDisplay.c:

Go to the source code of this file.

## Defines
#define | DISPLAY_bp 4
#define | BACKLIGHT_bp 5
## Functions
void | timer2_init (void)
| Initializes timer2.
int | main (void)
| ISR (TIMER2_OVF_vect)
## Variables
uint8_t | cnt = 0
uint8_t | cnt2 = 0
uint8_t | scroll
| scroll enable flag

## Detailed Description

UartDisplay Main File.

Authors:
  Dominic Rathje (dominic.rathje@uni-ulm.de)
  Christian Degenhart (christian.degenhart@uni-ulm.de)

Version:
  1.2

Note:
  - Compiler : WinAVR 20100110
  - Supported devices : ATMega8

Definition in file UartDisplay.c.

## Function Documentation

void timer2_init | ( | void | ) | `[inline]`

Initializes timer2.

- Prescaler is set to 1024
- Overflow Interrput enabled.

Definition at line 53 of file UartDisplay.c.